{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["app","按键","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"app","index":0,"n_rows":24,"n_cols":4,"rows_kept":24,"merged":[[1,0,5,0],[6,0,10,0],[11,0,23,0]],"flags":["formulas_cached_only"]}
[null,"按键","功能描述","注意事项"]
["首页","自动","门进入自动模式","1 进入自动运行模式\n2 门体是关闭状态保持不动\n3 门体是开启状态时发送关闭命令"]
[null,"常开","进入常开模式，并将门打开","1 发送开门命令\n2 进入常开模式，此时按键除停止外均失效\n3 这个时候不再处理碰撞，力量一直持续到开门为止\n4 注意门在开的过程中强行推门会造成电机过载保护"]
[null,"常闭","进入常闭模式，并将门关闭","1 发送关门命令\n2 进入常闭模式，此时按键除停止外均失效\n3 这个时候不再处理碰撞，力量一直持续到开门为止\n4 注意门在开的过程中强行推门会造成电机过载保护。"]
[null,"停止","门立刻停止，无论在什么状态下。","1 门体停止运行\n2 保持原工作模式（常开、常闭、自动）"]
[null,"连接设备","选择要连接的蓝牙设备","进入设备选择页面"]
["用户设置","开门速度","设置开门速度，1档最慢，5档最快，默认3档","注意每次设置会重置两端的缓冲距离"]
[null,"关门速度","设置关门速度，1档最慢，5档最快，默认3档","注意每次设置会重置两端的缓冲距离"]
[null,"开门停留时间","自动打开时，设置自动关门停留时间"]
[null,"电锁开关","设置电锁是否使能","开启使能是在关门后控制器自动打开电锁"]
[null,"运行模式","设置电机运行的模式状态","1 模式1为取消一切特殊设置\n2 为后期预留的接口\n注意该模式设置完需要重启电机"]
["工程设置","学习阶段出力系数","在开机学习阶段电机力量等级","1 5级为最大，1级最小，默认3级可以适用大多数的场景\n2 在学习阶段设置该参数双门不会自动同步"]
[null,"运行阶段出力系数","在正常运行阶段电机力量等级","1 5级为最大，1级最小，默认3级可以适用大多数的场景\n2 在学习阶段设置该参数双门不会自动同步\n3 1,2,3档在速度提升后会启动节能降低推力。4,5档会关闭节能，推力从头至尾都不变。"]
[null,"温度报警设置","设置电机保护报警温度","1 设置温度在80-110之间，默认值90可以适用大多数场景\n2 在学习阶段设置该参数双门不会自动同步"]
[null,"关门保持设置","关闭后使用电磁力保存门的位置","1 在学习阶段设置该参数双门不会自动同步\n2 一旦开启，开关门均有效"]
[null,"门长度设置","对于较小的门需要设置门的长度","1 小门针对特殊场景，一般无需设置\n2 小电机在门体70cm以上设置为70\n3 大电机在门体80cm以上设置为80\n4 其他特长电机设置为最大值\n"]
[null,"最大电流设置","设置点击保护报警电流值","最新门控产品升级了更先进的算法可以自动调整电流报警值，无需设置"]
[null,"开门方向选择","设置开门方向","在学习阶段设置该参数双门不会自动同步"]
[null,"多门设置","多个门联动时设置门编号","1 控制器经过升级，可以自动识别普通双门对开，普通单开和双开都无需设置\n2 该命令仅对多门联动有效"]
[null,"更改密码","更改连接密码","在任何阶段该命令均不会自动同步（同步存在安全隐患）\n设置完必须断开设备重新连接"]
[null,"一压设置","自动关门时按住门体约6秒，控制器即保持开门状态"]
[null,"遇阻灵敏度","调整运行时遇到障碍物时做出反应的灵敏度","1 5级为最不灵敏，1级最灵敏，默认3级可以适用大多数的场景\n2 在学习阶段设置该参数双门不会自动同步"]
[null,"电锁端缓冲","设置电锁出线端减速距离","1 每个控制器和挂载的门参数不能完全相同，该参数无论是学习还是正常使用时，均不支持双门自动同步\n2 为了安全每次设置速度均会重置缓冲距离\n3 考虑到安全因素，出厂设置缓冲距离稍长一点，可以自行适当减少，调整这个参数需注意碰撞"]
[null,"电源端缓冲","设置电源出线端减速距离","注意事项见上一条"]

{"sheet":"按键","index":1,"n_rows":6,"n_cols":4,"rows_kept":6,"flags":["formulas_cached_only"]}
["按键","颜色","功能描述","详细逻辑"]
["停止","黄","门停止运行","最高优先级，门体在运动状态时立刻停止"]
["开门（自动）","绿","开门停留设定时间后自动关门","APP自动模式下，在门体开启后并且经过等待时间后自动关门"]
["锁","蓝","关门上锁使能","按下后电锁启用，在下一次门体关闭后电锁自动打开。再按取消该功能。"]
["关门","棕","按下关门","APP自动模式下，按下就关门"]
["安全光线","白","关门过程中触发会将门打开","在门活动的过程中，有信号触发就开门。关门后失效"]

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}